[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 23: Automatic Search does Not Work. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 23: Automatic Search does Not Work.
DIAGNOSIS PROCEDURE
STEP 1. Check that the "APS" (automatic search) button be depressed properly. NOTE: When the time between songs on a tape is less than three seconds, or when there is a three second period in the middle of a song in which the volume level is extremely low, the automatic search function may not work properly. Q: Can the "APS" (automatic search) button be depressed properly? YES: Go to Step 2. NO: The button is operated improperly. Repair radio and tape player.
STEP 2. Check that the player works when the tape is changed. NOTE: Ensure that the tape label is not loose, that the tape itself is not deformed and that the tape is tightly wound. Also, tapes of C-120 or greater length often get caught in the mechanism and should not be used. Q: Does the player work if the tape is changed? YES: The tape used is defective. NO: Replace the radio and tape player. Check that the automatic search function operates normally.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 23: Automatic Search does Not Work. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation