[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - MAGNETIC CLUTCH TEST | PRINT PAGE / INDEX / PRIOR / NEXT

| MAGNETIC CLUTCH TEST Disconnect the magnetic clutch connector to the magnetic clutch.
| Connect positive battery voltage directly to the connector for the magnetic clutch. If the magnetic clutch is normal, there will be a "click." If the pulley and armature do not make contact ("click"), there is a malfunction.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - MAGNETIC CLUTCH TEST | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation