[55B] AUTOMATIC AIR CONDITIONER - - AIR MIXING DOOR MOTOR, AIR OUTLET CHANGEOVER DAMPER MOTOR AND BLOWER MOTOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| CHECK THE AIR MIXING DOOR CONTROL MOTOR AND POTENTIOMETER
CHECK THE AIR MIXING DOOR CONTROL MOTOR
Battery connection (+) terminal | Battery connection (-) terminal | Lever operation
1 | 3 | Rotate to the HOT position.
3 | 1 | Rotate to the COOL position.
Potentiometer check When the resistances between terminals 2 and 5 as well as terminals 5 and 6 are measured at the air mixing door motor check, the resistance value should change gradually within the standard value. Standard value: Approximately 0.65(MAX COOL) - 5.35(MAX HOT) kΩ
| MODE SELECTION DAMPER CONTROL MOTOR AND POTENTIOMETER CHECK
MODE SELECTION DAMPER CONTROL MOTOR CHECK
Battery connection (+) terminal | Battery connection (-) terminal | Lever operation
1 | 3 | Rotate to the DEF position.
3 | 1 | Rotate to the FACE position.
| Potentiometer check When the resistances between terminals 2 and 5 as well as terminals 5 and 6 are measured at the mode selection damper control motor check, the resistance value should change gradually within the standard value. Standard value: Approximately 0.65(DEF position) - 5.35(FACE position) kΩ
| BLOWER MOTOR CHECK Execute actuator test item No.01 to 04 by using MUT-II with the vehicle body, and check that the blower motor works normally (Refer to ).

[55B] AUTOMATIC AIR CONDITIONER - - AIR MIXING DOOR MOTOR, AIR OUTLET CHANGEOVER DAMPER MOTOR AND BLOWER MOTOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation