[55B] AUTOMATIC AIR CONDITIONER - - ROOM TEMPERATURE SENSOR AND HEATER WATER TEMPERATURE SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| INTERIOR TEMPERATURE SENSOR CHECK
| Check to see that the resistance shown in the graph is almost satisfied when measuring the resistance between the terminals under two or more different temperature conditions.
| HEATER WATER TEMPERATURE SENSOR CHECK
| Check to see that the resistance shown in the graph is almost satisfied when measuring the resistance between the terminals under two or more different temperature conditions.

[55B] AUTOMATIC AIR CONDITIONER - - ROOM TEMPERATURE SENSOR AND HEATER WATER TEMPERATURE SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation