[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER UNIT, HEATER CORE, BLOWER ASSEMBLY AND EVAPORATOR UNIT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

HEATER UNIT, HEATER CORE, BLOWER ASSEMBLY AND EVAPORATOR UNIT

REMOVAL AND INSTALLATION
WARNING When removing and installing the heater unit, do not let it bump against the SRS-ECU or the components.
Pre-removal and Post-installation Operation Refrigerant draining and Refilling (Refer to Charging and Discharging ). Engine coolant Draining and Refilling (Refer to GROUP 14, On vehicles service ). Instrument Panel Removal and Installation (Refer to GROUP 52A, Instrument Panel <L.H.drive vehicles> or <R.H.drive vehicles>). Air cleaner cover and air flow sensor assembly Removal and Installation (Refer to GROUP 15, Air cleaner <2400-except MIVEC>, <2400-MIVEC>).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Intake duct
|  | 2. | Joint duct
|  | 3. | Blower assembly
|  | 4. | Foot duct <front passenger's side>
|  | 5. | Front deck crossmember
|  | 6. | Heater hose connection
<<A>> |  | 7. | Liquid pipe B connection
<<A>> |  | 8. | Flexible suction hose connection
|  | 9. | O ring
|  | 10. | Centre duct
|  | 11. | Foot duct <driver's side>
|  | 12. | Heater case
| REMOVAL SERVICE POINT
| <<A>> FLEXIBLE SUCTION HOSE AND LIQUID PIPE B DISCONNECTION CAUTION As the compressor oil and receiver are highly moisture absorbent, use a non-porous material to plug the hose and nipples. To prevent the entry of dust or other foreign bodies, plug the dismantled hose and the nipples of the expansion valves.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER UNIT, HEATER CORE, BLOWER ASSEMBLY AND EVAPORATOR UNIT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation