[23A] AUTOMATIC TRANSMISSION (FF) - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
A/T fluid temperature sensor resistance kΩ | At 0°C | 16.7 - 20.5
At 20°C | 7.3 - 8.9
At 40°C | 3.4 - 4.2
At 60°C | 1.9 - 2.2
At 80°C | 1.0 - 1.2
At 100°C | 0.57 - 0.69
Damper clutch control (DCC) solenoid valve coil resistance (at 20°C) Ω | 2.7 - 3.4
Low & reverse (LR) solenoid valve coil resistance (at 20°C) Ω | 2.7 - 3.4
Second (2ND) solenoid valve coil resistance (at 20°C) Ω | 2.7 - 3.4
Underdrive (UD) solenoid valve coil resistance (at 20°C) Ω | 2.7 - 3.4
Overdrive (OD) solenoid valve coil resistance (at 20°C) Ω | 2.7 - 3.4
Reduction (RED) solenoid valve coil resistance (at 20°C) Ω <5A/T> | 2.7 - 3.4
Steering shift switch Ω <5A/T> | Upshift and hold | 990 - 1,010
Downshift and hold | 388 - 396
Stall speed r/min | 4G63-SOHC | 2,100 - 2,600
4G63-DOHC | 3,200 - 3,700
4G64, 4G69 | 2,400 - 2,900
Line pressure MPa | 1.01 - 1.05
Protruding length of stabilizer link mm | 22 ± 1.5

[23A] AUTOMATIC TRANSMISSION (FF) - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation