[26] FRONT AXLE - - SPECIFICATION(S) - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

LUBRICANTS
Item | Specified lubricant | Quantity
--- | --- | ---
PTJ boot grease | Repair kit grease | <2000-Non-Turbo> | 215 ± 10 g
<2000-Turbo> | 220 ± 10 g
<2400> | 150 ± 10 g
BJ boot grease | Repair kit grease | <2000-Non-Turbo> | 120 ± 10 g
<2000-Turbo> | 95 ± 10 g
<2400> | 85 ± 10 g
Dust seal inner grease | Repair kit grease | 14 - 20 g
Dust seal outer grease | Repair kit grease | 8 - 12 g

[26] FRONT AXLE - - SPECIFICATION(S) - LUBRICANTS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation