[54B] SMART WIRING SYSTEM (SWS) - - MULTI-DISTRIBUTION INPUT/OUTPUT BY CIRCUIT | PRINT PAGE / INDEX / PRIOR / NEXT

MULTI-DISTRIBUTION INPUT/OUTPUT BY CIRCUIT
Multi-distribution is employed by the following circuits. The relation of the input switches, sensors, ECUs connected by multi-distribution lines, and outputs are also shown below.
Buzzer Lamp still ON reminder warning function
Power window <Vehicles for Hong Kong spec. and Argentina> Power window timer function
Windshield wiper washer Windshield mist wiper Vehicle speed-dependent variable windshield intermittent wiper Windshield low speed wiper Windshield high speed wiper Windshield washer
Rear wiper washer Rear wiper Rear washer
Lighting Headlamp, tail lamp Headlamp automatic shutdown function <Except vehicles for Australia and New Zealand-2400> Auto lamp function <Vehicles for Hong Kong spec.> Wiper-linked auto lamp function <Vehicles for Hong Kong spec.> Front and rear fog lamp
Flasher Turn signal lamp Hazard warning lamp
Sunroof <Vehicles with sunroof> Sunroof timer function

[54B] SMART WIRING SYSTEM (SWS) - - MULTI-DISTRIBUTION INPUT/OUTPUT BY CIRCUIT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation