[00] GENERAL - - SUPPORT LOCATIONS FOR LIFTING AND JACKING | PRINT PAGE / INDEX / PRIOR / NEXT

SUPPORT LOCATIONS FOR LIFTING AND JACKING
SUPPORT POSITIONS FOR A GARAGE JACK, AXLE STANDS, SINGLE-POST LIFT OR DOUBLE-POST LIFT AND PLATE TYPE LIFT CAUTION Do not support the vehicles at locations other than specified supporting points. Doing so will cause damage, etc.
GARAGE JACK CAUTION Never support any point other than the specified one, or that point will be deformed.
AXLE STANDS AND A SINGLE-POST LIFT OR DOUBLE-POST LIFT CAUTION If rubber attachments with grooves that are too thick are used at the front support positions, the front fender may become bent, so be sure to use rubber attachments with groove thicknesses of 18 mm or less. If attachments which are not high enough are used, they may damage areas such as the side step. Be sure to use attachments which are high enough, or remove the side step if not using attachments.
PLATE TYPE LIFT CAUTION To avoid damaging the side sill garnish, put a wooden block between the side sill and a lift. Support the side sill flange with a lift.

[00] GENERAL - - SUPPORT LOCATIONS FOR LIFTING AND JACKING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation