[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - A/T FLUID TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| A/T FLUID TEMPERATURE SENSOR CHECK Drain the A/T fluid and remove the valve body cover.
| Remove the A/T fluid temperature sensor.
| Measure the resistance between A/T control solenoid valve assembly connector terminals 1 and 2. Standard value:
A/T fluid temperature (°C) | Resistance value (Ω)
--- | ---
0 | 16.7 - 20.5
20 | 7.3 - 8.9
40 | 3.4 - 4.2
60 | 1.9 - 2.2
80 | 1.0 - 1.2
100 | 0.57 - 0.69
NOTE: The N range indicator <Vehicles for Hong Kong spec.> or A/T fluid temperature warning lamp <Except for Hong Kong spec.> on the combination meter flashes when the temperature reaches approximately 125 °C or higher and then stops flashing when the temperature drops below approximately 115°C. If the A/T fluid temperature sensor resistance and the temperature when the N range indicator is flashing or switched off are outside the standard value ranges, replace the A/T fluid temperature sensor.

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - A/T FLUID TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation