[55A] HEATER, AIR CONDITIONER AND VENTILATION - - CONDENSER AND CONDENSER FAN MOTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

CONDENSER AND CONDENSER FAN MOTOR

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Refrigerant draining and Refilling (Refer to Charging and Discharging ). Air cleaner cover and air flow sensor assembly Removal and Installation (Refer to GROUP 15, Air cleaner <2400-except MIVEC>, <2400-MIVEC>).
|  |  | Condenser removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Liquid pipe A connection
<<A>> |  | 2. | Flexible discharge hose connection
|  | 3. | O ring
| >>A<< | 4. | Condenser assembly
|  | 5. | Receiver
|  | 6. | Clamp
|  | 7. | O ring
|  | 8. | Condenser
|  |  | Fan shroud assembly removal steps
|  | 9. | Fan shroud assembly
|  | 10. | Fan
|  | 11. | Fan motor
|  | 12. | Fan shroud
|  |  | Air guide panel removal steps
|  | • | Front bumper (Refer to 51, Front bumper <2000>, <2400>).
|  | 13. | Air guide panel
| REMOVAL SERVICE POINT
| <<A>> FLEXIBLE SUCTION HOSE AND LIQUID PIPE A DISCONNECTION CAUTION As the compressor oil and receiver are highly moisture absorbent, use a non-porous material to plug the hose and nipples. To prevent the entry of dust or other foreign bodies, plug the dismantled hose and condenser assembly nipples.
| INSTALLATION SERVICE POINT
| >>A<< CONDENSER INSTALLATION When replacing the condenser, refill it with a specified amount of compressor oil and install it. (to the vehicle). Compressor oil: SUN PAG 56 Quantity: 15 mL

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - CONDENSER AND CONDENSER FAN MOTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation