[54A] CHASSIS ELECTRICAL - - COLUMN SWITCH - COLUMN SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| WINDSHIELD WIPER AND WASHER SWITCH CHECK <L.H. DRIVE VEHICLES>
Switch position | Tester condition | Specified condition
--- | --- | ---
OFF | 4 - 6, 5 - 6, 6 - 7, 6 - 8, 6 - 9, 6 - 10, 6 - 11 | Open circuit
Windshield mist wiper switch | 6 - 11 | Less than 2 ohms
Windshield intermittent wiper switch | 6 - 10 | Less than 2 ohms
Windshield low-speed wiper switch | 6 - 9 | Less than 2 ohms
Windshield high-speed wiper switch | 6 - 8 | Less than 2 ohms
Windshield washer switch | 6 - 7 | Less than 2 ohms
Rear wiper switch | 4 - 6 | Less than 2 ohms
Rear washer switch | 5 - 6 | Less than 2 ohms
NOTE: Measure intermittent volume switch resistance value between terminals 3 and 6. The measured resistance should change smoothly from approximately 0 ohm ("FAST" position) to 1 kiloohm ("SLOW" position) On L.H.drive vehicles, integrated column ECU does not allow turn-signal and lighting switch continuity test. For inspection and diagnosis, refer to the respective Group below. Not using SWS monitor: GROUP 54B, Troubleshooting . Using SWS monitor: GROUP 54C, Troubleshooting .
| TURN-SIGNAL AND LIGHTING SWITCH CHECK <R.H. DRIVE VEHICLES>
Switch position | Tester condition | Specified condition
--- | --- | ---
OFF | 3 - 4, 3 - 6, 3 - 7, 3 - 8, 3 - 9, 3 - 10, 3 - 11 | Open circuit
Headlamp washer switch | 3 - 4 | Less than 2 ohms
Headlamp switch | 3 - 6 | Less than 2 ohms
Tail lamp switch | 3 - 7 | Less than 2 ohms
Passing switch | 3 - 8 | Less than 2 ohms
Dimmer switch | 3 - 9 | Less than 2 ohms
Turn-signal lamp switch (RH) | 3 - 10 | Less than 2 ohms
Turn-signal lamp switch (LH) | 3 - 11 | Less than 2 ohms
NOTE: On R.H.drive vehicles, integrated column ECU does not allow windshield wiper switch continuity test. For inspection and diagnosis, refer to the respective Group below. Not using SWS monitor: GROUP 54B, Troubleshooting . Using SWS monitor: GROUP 54C, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - COLUMN SWITCH - COLUMN SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation