[37] POWER STEERING - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB991897 | Ball joint remover | Knuckle and tie rod end ball joint disconnection NOTE: Steering linkage puller (MB990635 or MB991113) is also available to disconnect knuckle and tie rod end ball joint.
| MB990326 | Preload socket | Tie rod end ball joint starting torque check
| MB991548 | Power steering oil pressure gauge adapter (Pump side) | Oil pump pressure test
| MB991549 | Power steering oil pressure gauge adapter (Hose side)
| MB990662 | Power steering oil pressure gauge
| MB990784 | Ornament remover | Cover removal
| MB990803 | Steering wheel puller | Steering wheel removal
| MB990228 or MB991006 | Preload socket | Steering gear total pinion torque check and adjustment
| MB991621 | Rack support cover wrench | Rack support adjustment Rack support cover removal
| MB990925 | Bearing and oil seal installer set | Oil seal and bearing installation MB990927, MB990938, MB990939 (For details, refer to GROUP 26, Special Tools .)
| MB991120 | Needle bearing puller | Needle roller bearing removal
| MB991199 | Oil seal and bearing installer | Oil seal installation
| MB991197 | Bar (long type)
| MB991202 | Oil seal and bearing installer | Needle bearing installation Lower bearing installation
| MB991213 | Rack installer | Rack installation
| MB991203 | Oil seal and bearing installer | Oil seal and bearing installation
| MB991317 | Seal ring installer | Seal ring installation
| MB990941 | Torque tube bearing installer | Lower oil seal installation
| MB991561 | Boot band crimping tool | Bellows band installation
| MB990776 | Front axle base | Tie rod end ball joint dust cover installation

[37] POWER STEERING - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation