[51] EXTERIOR - - MARK - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
|  | 1. | Front three-diamond mark
| >>A<< | 2. | Rear three-diamond mark
| >>A<< | 3. | 4WD <Option - Vehicles for Australia>, 4WD decal
| >>A<< | 4. | SPORT GEAR mark
| >>A<< | 5. | GLX, GLS mark
| >>A<< | 6. | OUTLANDER mark
| INSTALLATION SERVICE POINT
| >>A<< MARK INSTALLATION
| Clean the mark installation surfaces on the body with unleaded petrol. CAUTION When attaching the marks, the ambient temperature should be 20 - 38°C and the air should be completely free of dust. If the ambient temperature is lower than 20°C, the marks and the places on the vehicle body where the marks are to be attached should be heated to 20 - 38°C. Peel off the protection sheet on the back of the mark to paste it on the installation position.

[51] EXTERIOR - - MARK - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation