[36] PARKING BRAKES - - ON-VEHICLE SERVICE - LINING RUNNING-IN <Vehicles with rear drum-in disc brakes> | PRINT PAGE / INDEX / PRIOR / NEXT

| LINING RUNNING-IN <Vehicles with rear drum-in disc brakes> CAUTION Carry out running-in in a place with good visibility, and pay careful attention to safety. Carry out running-in by the following procedure when replacing the parking brake linings or the rear brake disc rotors, or when brake performance is insufficient.
| <L.H. drive vehicles> Adjust the parking brake lever stroke to the specified value. Specified value (Operation force: Approx. 200 N): 4 - 5 notches Hook a spring balance onto the centre of the parking brake lever grip and pull it with a force of 100 - 150 N in a direction perpendicular to the handle. Drive the vehicle at a constant speed of 35 - 50 km/h for 100 metres. Release the parking brake and let the brakes cool for 5 - 10 minutes. Repeat the procedure in steps 2 to 4 four or five times.
| <R.H. drive vehicles> Adjust the parking brake pedal stroke to the standard value. Specified value (Operation force: Approx. 200 N): 1 - 2 notches Depress the parking brake pedal by 100 to 150 N (equivalent to approximately one notch). Drive the vehicle at a constant speed of 35 - 50 km/h for 100 metres. Release the parking brake and let the brakes cool for 5 - 10 minutes. Repeat the procedure in steps 2 to 4 four or five times.

[36] PARKING BRAKES - - ON-VEHICLE SERVICE - LINING RUNNING-IN <Vehicles with rear drum-in disc brakes> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation