[11D] ENGINE OVERHAUL <4G6-DOHC> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

TORQUE SPECIFICATIONS
Item | N·m
--- | ---
ALTERNATOR AND IGNITION COIL
Oil level gauge guide bolt | 13 ± 1
Idler pulley bolt | 79 ± 5
Auto-tensioner assembly bolt (M8) | 24 ± 4
Auto-tensioner assembly bolt (M10) | 44 ± 10
Water pump pulley bolts | 8.8 ± 1.0
Alternator brace bolt (flange bolt) | 23 ± 3
Alternator brace bolts (washer assembled bolt) | 22 ± 4
Alternator nuts | 44 ± 10
Crankshaft pulley bolts | 25 ± 4
Center cover bolts | 3.0 ± 0.5
Ignition coil bolts | 10 ± 2
Spark plugs | 25 ± 5
SOLENOID AND VACUUM HOSE
Vacuum pipe and hose assembly bolts | 11 ± 1
EGR valve bolts | 20 ± 2
Engine hanger bolt | 19 ± 3
Solenoid valve assembly nut | 36 ± 6
Solenoid valve assembly bolts(M6) | 9.0 ± 1.0
Solenoid valve assembly bolts(M8) | 23 ± 4
TIMING BELT
Timing belt cover bolts (flange bolt) | 11 ± 1
Timing belt cover bolt (washer-assembled bolt) | 9.0 ± 1.0
Power steering pump bracket bolts | 49 ± 9
Tensioner pulley bolt | 48 ± 5
Tensioner arm bolt | 21 ± 4
Auto-tensioner bolts | 23 ± 3
Idler pulley bolt | 35 ± 6
Crankshaft angle sensor bolts | 8.8 ± 1.0
Oil pump sprocket nut | 54 ± 4
Crankshaft bolt | 167
Tensioner "B" bolt | 19 ± 3
Counterbalance shaft sprocket bolt | 45 ± 3
Rocker cover bolts | 3.5 ± 0.5
Engine support bracket bolts | 49 ± 5
Camshaft sprocket bolts | 88 ± 10
FUEL SYSTEM
Throttle body bolts | 19 ± 3
Fuel pressure regulator bolts | 9.0 ± 2.0
Delivery pipe and injector assembly bolts | 11 ± 1
INLET MANIFOLD
MDP sensor bolts | 5.0 ± 1.0
Inlet manifold stay bolts | 31 ± 3
Inlet manifold bolts (M8) | 20 ± 2
Inlet manifold bolts and nuts (M10) | 36 ± 6
Detonation sensor | 23 ± 2
EXHAUST MANIFOLD
Engine hanger bolt | 19 ± 3
Turbocharger heat protector bolts | 23 ± 3
Exhaust fitting bracket bolts | 36 ± 5
Exhaust fitting bolts | 59 ± 5
Air outlet fitting bolts | 19 ± 1
Oil return pipe bolts | 9.0 ± 1.0
Exhaust manifold heat protector bolts | 23 ± 3
Turbocharger assembly and pipe assembly bolts, nuts | 59 ± 5
Oil pipe bolt (flange bolt) | 11 ± 1
Oil pipe bolt (eye bolt M10) | 17 ± 2
Water pipe bolt (eye bolt M12) | 28 ± 5
Water pipe bolt (flange bolt) | 10 ± 1
Exhaust manifold nuts (M8) | 33 ± 6
Exhaust manifold nuts (M10) | 55 ± 10
WATER PUMP AND WATER HOSE
Engine coolant temperature sensor | 29 ± 10
Engine coolant temperature gauge unit | 10.8 ± 1.0
Water outlet fitting bolts | 13 ± 2
Water inlet fitting bolts | 13 ± 2
Thermostat housing bolts | 23 ± 4
Water inlet pipe bolt (M8) | 13 ± 2
Water pump bolts | 14 ± 1
ROCKER ARMS AND CAMSHAFTS
Camshaft position sensor bolt | 10 ± 1
Cover bolts | 10 ± 2
Camshaft position sensing cylinder bolt | 22 ± 4
Camshaft position sensor support bolts | 14 ± 1
Bearing cap bolts | 20 ± 1
Oil delivery body bolts | 11 ± 1
CYLINDER HEAD AND VALVES
Cylinder head bolts | 78 ± 2 → 0 → 20 ± 2 →+ 90°+ 90°
OIL PUMP CASE AND OIL PAN
Drain plug | 39 ± 5
Transmission stay bolts | 22 ± 4
Oil pan upper section bolts | 9.0 ± 3.0
Oil pan lower section bolts | 7.0 ± 1.0
Baffle plate bolt | 7.0 ± 1.0
Oil screen bolts | 19 ± 3
Oil pressure switch | 19 ± 3
Relief plug | 44 ± 5
Oil filter bracket bolts | 19 ± 3
Plug cap | 23 ± 3
Flange bolt | 36 ± 3
Oil pump case bolts | 23 ± 3
Oil pump cover bolts | 17 ± 1
Oil pump cover screw | 10 ± 2
PISTONS AND CONNECTING RODS
Connecting rod cap nuts | 20 ± 2 → 90° to 94°
CRANKSHAFT AND CYLINDER BLOCK
Drive plate bolts | 132 ± 5
Rear plate bolt | 11 ± 1
Bell housing cover bolts | 9.0 ± 1.0
Rear oil seal case bolts | 11 ± 1
Beam bearing cap bolts | 25 ± 2 → 90° to 100°

[11D] ENGINE OVERHAUL <4G6-DOHC> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation