[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW SAFETY MECHANISM CHECK <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

| POWER WINDOW SAFETY MECHANISM CHECK <VEHICLES FOR HONG KONG SPEC AND ARGENTINA>
| Place a wooden board about 10 mm thick as shown. Then, raise the window glass. Check that the window lowers by about 150 mm when the window clamps the board. If this doesn’t happen, carry out troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . NOTE: If the anti-trap function (safety mechanism) is activated consecutively three times or more, make the power window switch learn the fully closed position of the power window (Refer to ).

[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW SAFETY MECHANISM CHECK <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation