[36] PARKING BRAKES - - PARKING BRAKE LINING AND DRUM <Vehicles with rear drum-in disc brakes> - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| PARKING BRAKE LINING AND BRAKE DRUM CHECK
| Measure the thickness of the brake lining at several places. Standard value: 2.8 mm Minimum Limit: 1.0 mm If the thickness of the brake lining is below the limit, replace the shoe and lining assemblies on both sides of the vehicle. Never replace only one side.
| Measure the inside diameter of the brake disc in two places or more. Standard value: 168.0 mm Limit: 169.0 mm If the inside diameter exceeds the limit, or if it is excessively worn on one side, replace the brake disc.

[36] PARKING BRAKES - - PARKING BRAKE LINING AND DRUM <Vehicles with rear drum-in disc brakes> - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation