[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - CHECK CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK CHART FOR TROUBLE SYMPTOMS
Trouble | Inspection procedure No. | Reference page
--- | --- | ---
Communication with MUT-II/III is not possible (Communication with all systems is not possible). | - | 4G63: GROUP 13A - Troubleshooting 4G64: GROUP 13B - Troubleshooting 4G69: GROUP 13C - Troubleshooting
Communication with MUT-II/III is not possible (Communication is not possible with SRS). | 1 |
When the ignition switch is turned to the "ON" position (engine stopped), the SRS warning lamp does not illuminate. | Refer to diagnosis code No.43. |
After the ignition switch is turned to the "ON" position, the SRS warning lamp does not go off within approximately seven seconds. | Refer to diagnosis code No.43. |

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - CHECK CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation