[27B] REAR AXLE <4WD> - - DRIVE SHAFT ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION Check the drive shaft for damage, bending or corrosion. Check the drive shaft spline part for wear or damage. Check the boots for deterioration, damage or cracking. Check the dust cover for damage or deterioration.

[27B] REAR AXLE <4WD> - - DRIVE SHAFT ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation