[27B] REAR AXLE <4WD> - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIFICATION(S)

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Rear axle total backlash mm | - | 5
Wheel bearing rotation starting torque N·m | - | 1.0
Wheel bearing axial play mm | - | 0.05
TJ boot assembly dimension mm | 2000-Turbo | 90 ± 3 | -
2400 | 80 ± 3 | -
Drive gear backlash mm | 0.11 - 0.16 | -
Drive gear runout mm | - | 0.05
Differential gear backlash mm | 0 - 0.076 | 0.2
Drive pinion turning torque N·m | Without oil seal | 0.9 - 1.2 | -
With oil seal | Companion flange (oil seal contacting area) with anti-rust agent | 1.0 - 1.3 | -
Companion flange (oil seal contacting area) with gear oil applied | 0.5 - 0.6 | -

[27B] REAR AXLE <4WD> - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation