[37] POWER STEERING - - ON-VEHICLE SERVICE - FLUID REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| FLUID REPLACEMENT Raise and support the front wheels.
| Disconnect the return hose connection, and then connect a vinyl hose to the return hose, and drain the fluid into a container. Disconnect the ignition coil connectors. (Refer to GROUP 16, Ignition Coil <2000-SOHC>, <2000-DOHC>, <2400>.) While operating the starter motor intermittently, turn the steering wheel all the way to the left and right several times to drain all of the fluid. Connect the return hose securely, and then secure with the clip. Fill the oil reservoir with specified fluid up to the lower position of the filler, and then bleed the air. Specified fluid: ATF DEXRON III or DEXRON II

[37] POWER STEERING - - ON-VEHICLE SERVICE - FLUID REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation