[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR OUTSIDE HANDLE PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| DOOR OUTSIDE HANDLE PLAY CHECK
| Check that the door outside handle play is within the standard value range. Standard value (A): Front door: 0 - 3.9 mm (Target value: 1.9 mm) Rear door: 0 - 3.6 mm (Target value: 1.6 mm) If the door outside handle play is not within the standard value range, check the door outside handle or the door latch assembly. Replace if necessary. Refer to .

[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR OUTSIDE HANDLE PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation