[51] EXTERIOR - - WIPER AND WASHER - WINDSHIELD WIPER AND WASHER | PRINT PAGE / INDEX / PRIOR / NEXT

WIPER AND WASHER

WINDSHIELD WIPER AND WASHER
WASHER NOZZLE The windshield washer is a 2 nozzle, 4 jet type. It also features a washer interlocked wiper function.
WIPER LINK ASSEMBLY Employment of a module structure wiper link assembly has increased durability of the wiper link area, provides smoother wiper operations and quieter wiper operations.
INTERMITTENT WIPER The intermittent wiper features a vehicle speed sensitive intermittent time variable system. The vehicle speed sensitive intermittent function can be turned OFF. It is factory preset (default setting) to ON.
NOTE: Refer to Group 54B, SWS <Hong Kong spec.> or <Except for Hong Kong spec.> to change the functions.
MIST WIPER FUNCTION Features a mist wiper function that rigorously wipes away rain with high speed wiping when the mist switch is ON, slows down when the mist switch is OFF and operates until stopped. When the mist switch is temporarily turned ON the wiper wipes once at low speed.
CONSTRUCTION DIAGRAM

[51] EXTERIOR - - WIPER AND WASHER - WINDSHIELD WIPER AND WASHER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation