[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 36. HOSES, FLUID LINES AND CONNECTIONS LOCATED UNDER HOOD | PRINT PAGE / INDEX / PRIOR / NEXT

| 36. HOSES, FLUID LINES AND CONNECTIONS LOCATED UNDER HOOD
| Check all brake, fuel, power steering and air conditioner lines and connections; verify proper routing, check connections for leaks, tighten loose connector as required. Inspect routing and connections of all vacuum, and radiator and heater houses. CAUTION Remember that the air conditioner system is under pressure. NOTE: Keep in mind that an oily residue around an air conditioner connector does not necessarily indicate a leak. Oil is used to lubricate fittings during assembly. Be sure lines are not twisted or kinked.

[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 36. HOSES, FLUID LINES AND CONNECTIONS LOCATED UNDER HOOD | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation