[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - ROOF LID GLASS OPERATION CURRENT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ROOF LID GLASS OPERATION CURRENT CHECK
| Remove the fuse of the sunroof, then connect the circuit tester as shown in the Figure. Turn ON the sunroof switch, then measure the operating current of the intermediary segment when the sunroof is moving, with the sunroof fully closed, when the sunroof is fully opened and when the sunroof is tilted fully up. Standard value: 7 A or less (at 20 °C) Check the following areas if the operating current of exceeds the standard value. Sunroof installation, deformation and appearance of any foreign substances. Drive cable installation. Tilting of roof lid glass.

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - ROOF LID GLASS OPERATION CURRENT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation