[3] WELDED PANEL REPLACEMENT - - FRONT SIDEMEMBER (PARTIAL REPLACEMENT) | PRINT PAGE / INDEX / PRIOR / NEXT

FRONT SIDEMEMBER (PARTIAL REPLACEMENT)
NOTE: Refer to the Headlamp Support section on for the welding point with headlamp support.
| NOTE ON REPAIR WORK
| REMOVAL
| Remove the battery bracket front on the cut area in advance when cutting the front sidemember inner.
| As shown in the figure of the instructions, bend the front fender shield on the cut area in advance, when cutting the front sidemember outer.
| INSTALLATION
| Remove the battery bracket front from the new front sidemember inner.
| Assemble the front sidemember, then assemble the battery bracket front in the location of the figure of the instructions, then return the front fender shield bent back to the original state.

[3] WELDED PANEL REPLACEMENT - - FRONT SIDEMEMBER (PARTIAL REPLACEMENT) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation