[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - WHEEL BEARING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| WHEEL BEARING AXIAL PLAY CHECK Remove the hub cap and brake drum.
| Check the bearing's axial play. Place a dial gauge against the hub surface; then move the hub in the axial direction and check whether or not there is axial play. Limit: 0.05 mm If the play exceeds the limit, the self-locking nut should be tightened to the specified torque and check the axial play again. Tightening torque: 175 ± 25 N·m Replace the rear hub assembly if an adjustment cannot be made to within the limit.

[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - WHEEL BEARING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation