[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR DIAGNOSIS CODE
Code No. | Diagnosis item | Reference page
--- | --- | ---
P0100 | Air flow sensor system |
P0105 | Barometric pressure sensor system <Vehicles except for Hong kong> |
P0105 | Manifold absolute pressure sensor system |
P0110 | Intake air temperature sensor system |
P0115 | Engine coolant temperature sensor system |
P0122* | Throttle position sensor (main) circuit low input |
P0123* | Throttle position sensor (main) circuit high input |
P0125* | Feedback system monitor <Vehicles for Hong kong> |
P0130 | Cylinder 1, 4 oxygen sensor (front) system <Vehicles for Hong kong> |
P0135 | Cylinder 1, 4 oxygen sensor (front) heater system <Vehicles for Hong kong> |
P0136 | Cylinder 1, 4 oxygen sensor (rear) system <Vehicles for Hong kong> |
P0141 | Cylinder 1, 4 oxygen sensor (rear) heater system <Vehicles for Hong kong> |
P0150 | Cylinder 2, 3 oxygen sensor (front) system <Vehicles for Hong kong> |
P0155 | Cylinder 2, 3 oxygen sensor (front) heater system <Vehicles for Hong kong> |
P0156 | Cylinder 2, 3 oxygen sensor (rear) system <Vehicles for Hong kong> |
P0161 | Cylinder 2, 3 oxygen sensor (rear) heater system <Vehicles for Hong kong> |
P0170 | Abnormal fuel system (cylinder 1, 4) <Vehicles for Hong kong> |
P0173 | Abnormal fuel system (cylinder 2, 3) <Vehicles for Hong kong> |
P0201 | No. 1 injector system |
P0202 | No. 2 injector system |
P0203 | No. 3 injector system |
P0204 | No. 4 injector system |
P0222* | Throttle position sensor (sub) circuit low input |
P0223* | Throttle position sensor (sub) circuit high input |
P0300* | Ignition coil (power transistor) system <Vehicles except for Hong kong> |
P0300* | Random/multiple cylinder misfire detected <Vehicles for Hong kong> |
P0301* | No. 1 cylinder misfire detected <Vehicles for Hong kong> |
P0302* | No. 2 cylinder misfire detected <Vehicles for Hong kong> |
P0303* | No. 3 cylinder misfire detected <Vehicles for Hong kong> |
P0304* | No. 4 cylinder misfire detected <Vehicles for Hong kong> |
P0325 | Detonation sensor system |
P0335 | Crank angle sensor system |
P0340 | Camshaft position sensor system |
P0403 | Exhaust gas recirculation control system |
P0421 | Warm Up Catalyst Malfunction (cylinder 1, 4) <Vehicles for Hong kong> |
P0431 | Warm Up Catalyst Malfunction (cylinder 2, 3) <Vehicles for Hong kong> |
P0443 | Purge control solenoid valve system <Vehicles for Hong kong> |
P0500 | Vehicle speed signal system <Vehicles for Hong kong> |
P0505 | Idle speed control (ISC) system |
P0513 | Immobilizer malfunction |
P0551* | Power steering fluid pressure switch system <Vehicles for Hong kong> |
P0554 | Power steering fluid pressure switch circuit intermittent <Vehicles for Hong kong> |
P0603 | EEPROM malfunction |
P0606* | Engine-A/T-ECU main processor malfunction <Vehicles except for Hong kong> |
P0622 | Alternator FR terminal system |
P0638* | Throttle valve control servo circuit range/performance problem |
P0642* | Throttle position sensor power supply |
P0657* | Throttle valve control servo relay circuit malfunction |
P1021 | Oil control valve |
P1602* | Communication malfunction (between engine-A/T-ECU main processor and system LSI) |
P1603* | Battery backup circuit malfunction <Vehicles for Hong kong> |
P1751* | A/T control relay system | A/T DTC No. 54 (A/T control relay system) |
P2100* | Throttle valve control servo circuit (open) |
P2101* | Throttle valve control servo magneto malfunction |
P2102* | Throttle valve control servo circuit (shorted low) |
P2103* | Throttle valve control servo circuit (shorted high) |
P2121* | Accelerator pedal position sensor (main) circuit range/performance problem <Vehicles except for South africa, GCC and Australia> |
P2122* | Accelerator pedal position sensor (main) circuit low input |
P2123* | Accelerator pedal position sensor (main) circuit high input |
P2126* | Accelerator pedal position sensor (sub) circuit range/performance problem <Vehicles except for South africa, GCC and Australia> |
P2127* | Accelerator pedal position sensor (sub) circuit low input |
P2128* | Accelerator pedal position sensor (sub) circuit high input |
P2135* | Throttle position sensor (main and sub) range/performance problem |
P2138* | Accelerator pedal position sensor (main and sub) range/performance problem |
P2173* | Abnormal intake air amount |
NOTE: Do not replace the engine-A/T-ECU until a through terminal check reveals there are no short/open circuit. Check that the engine-A/T-ECU earth circuit is normal before checking for the cause of the problem. After the engine-A/T-ECU has detected a malfunction, a diagnosis code is recorded the next time the engine is started and the same malfunction is re-detected. However, for items marked with "*", the diagnosis code is recorded on the first detection of the malfunction.

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation