[15] INTAKE AND EXHAUST - - INLET MANIFOLD - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G63-DOHC>
Pre-removal Operation Fuel Line Pressure Reduction [Refer to GROUP 13A, On-vehicle Service - Fuel Pump Connector Disconnection (How to Reduce Pressurized Fuel Lines) .] Throttle Body Removal (Refer to GROUP 13A, Throttle Body ). | Post-installation Operation Throttle Body Installation (Refer to GROUP 13A, Throttle Body ). Accelerator Cable Adjustment (Refer to GROUP 17, On-vehicle Service - Accelerator Cable Check and Adjustment ). Fuel Leak Check
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Manifold differential pressure sensor connector
|  | 2. | Purge control solenoid valve connector
|  | 3. | EGR control solenoid valve connector
|  | 4. | Detonation sensor connector
|  | 5. | Injector connectors
|  | 6. | Waste gate solenoid valve connector
|  | 7. | Fuel pressure control solenoid valve connector
|  | 8. | Accelerator cable connection
|  | 9. | Manifold differential pressure sensor
|  | 10. | O-ring
|  | 11. | Emission control equipment hose connection
| >>A<< | 12. | Fuel high-pressure hose connection
|  | 13. | O-ring
|  | 14. | Fuel return line hose connection
<<A>> |  | 15. | Fuel delivery pipe and fuel injector assembly
|  | 16. | Insulators
|  | 17. | Vacuum hose connection
|  | 18. | Oil level gauge and guide
|  | 19. | O-ring
|  | 20. | Detonation sensor connector clamp
|  |  | Removal steps
--- | --- | --- | ---
|  | 21. | Vacuum hose and pipe assembly
|  | 22. | Engine hanger
|  | 23. | Solenoid valve assembly
|  | 24. | EGR valve
|  | 25. | EGR valve gasket
|  | 26. | Brake booster vacuum hose connection
|  | 27. | PCV hose
|  | 28. | Intake manifold stay
|  | 29. | Alternator brace stay
|  | 30. | Intake manifold assembly
|  | 31. | Intake manifold gasket
| REMOVAL SERVICE POINT
| <<A>> FUEL DELIVERY PIPE AND FUEL INJECTOR ASSEMBLY REMOVAL CAUTION Do not drop the injector. Remove the fuel delivery pipe with the fuel injector assembly attached to it.
| INSTALLATION SERVICE POINT
| >>A<< FUEL HIGH-PRESSURE HOSE INSTALLATION Apply a drop of new engine oil to the O-ring. Turn the fuel high-pressure hose to the right and left to install to the fuel delivery pipe. Be careful not to damage the O-ring. After installing, check that the item turns smoothly. If it dose not turn smoothly, the O-ring may be trapped, remove the item, re-install it into the fuel delivery pipe and check again. Tighten the fuel high-pressure hose to the specified torque. Tightening torque: 5.0 ± 1.0 N·m

[15] INTAKE AND EXHAUST - - INLET MANIFOLD - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation