[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - ON-VEHICLE SERVICE - RESISTIVE CORD CHECK <4G6-SOHC, 4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

| RESISTIVE CORD CHECK <4G6-SOHC, 4G6-DOHC>
| Measure the resistance of the all spark plug cables. Check cap and coating for cracks. Measure resistance. Limit: Maximum 19 kΩ

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - ON-VEHICLE SERVICE - RESISTIVE CORD CHECK <4G6-SOHC, 4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation