[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D2. CHECK FRONT WHEEL BEARINGS FOR PLAY | PRINT PAGE / INDEX / PRIOR / NEXT

| D2. CHECK FRONT WHEEL BEARINGS FOR PLAY Remove the disc brake caliper and suspend it with a wire. Remove the brake disc from the front hub.
| Attach a dial gauge as shown in the illustration, and then measure the axial play while moving the hub in the axial direction. Limit: 0.05 mm If axial play exceeds the limit, replace the front hub assembly.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D2. CHECK FRONT WHEEL BEARINGS FOR PLAY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation