[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - DETONATION SENSOR - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69>
CAUTION Do not drop or hit the detonation sensor against other components. Internal damage may result, and the detonation sensor will need to be replaced.
Pre-removal and Post-installation Operation Air Cleaner Removal and Installation (Refer to GROUP 15, Air Cleaner ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Detonation sensor connector connection
|  | 2. | Detonation sensor clamp
|  | 3. | Harness clamp
|  | 4. | Intake manifold stay
<<A>> | >>A<< | 5. | Detonation sensor
|  | 6. | Detonation sensor connector bracket
| REMOVAL SERVICE POINT
| <<A>> DETONATION SENSOR REMOVAL
| Use special tool detonation sensor wrench (MD998773) to remove the detonation sensor.
| INSTALLATION SERVICE POINT
| >>A<< DETONATION SENSOR INSTALLATION
| Use special tool detonation sensor wrench (MD998773) to tighten the detonation sensor to the specified torque.

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - DETONATION SENSOR - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation