[42] BODY - - MAIN BODY - QUIETNESS | PRINT PAGE / INDEX / PRIOR / NEXT

QUIETNESS Quietness has been improved with foam sound absorbent material and urethane foam. High rigidity foam material We have successfully lowered road noises by packing highly rigid form material in the front side (right-hand side) and rear side members to suppress panel vibration. Acoustic foam materials Noise intrusion is reduced by adding acoustic foam material to the front pillar, roof side rail, centre pillar, rear pillar, gate pillar and inside of the wheel house arch area. Urethane foam Noise intrusion is also reduced by inserting urethane foam inside the centre pillar.

[42] BODY - - MAIN BODY - QUIETNESS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation