[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

COMPONENT LOCATION
Name | Symbol | Name | Symbol
--- | --- | --- | ---
Accelerator pedal position sensor (with accelerator pedal position switch) | A | Engine control relay | I
A/C pressure sensor | A | Throttle valve control servo relay | I
Crank angle sensor | B | Oxygen sensor (front) <Except for Hong kong> | J
Detonation sensor | C | Cylinder 1,4 oxygen sensor (front) <Vehicles for Hong kong> | J
Manifold absolute pressure sensor | C | Oxygen sensor (rear) <Vehicles for Brazil and Chile> | K
Purge control solenoid valve | C | Cylinder 1,4 oxygen sensor (rear) <Vehicles for Hong kong> | L
Injector | D | Ignition coil | M
EGR valve | E | Cylinder 2,3 oxygen sensor (rear) <Vehicles for Hong kong> | N
Electronic-controlled throttle valve (Throttle position sensor and throttle valve control servo) | F | Cylinder 2,3 oxygen sensor (front) <Vehicles for Hong kong> | O
Inhibitor switch | P
Camshaft position sensor | G | Power steering fluid pressure switch | P
Oil control valve | G | Fuel pump relay (1) and (2) | Q
Camshaft position sensor | G | Engine warning lamp (check engine lamp) | R
Engine coolant temperature sensor | G | Diagnosis connector | S
Air flow sensor (with intake air temperature sensor) | H | A/C switch | T
A/C relay | I | Engine-A/T-ECU (with barometric pressure sensor) | U

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation