[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - ESSENTIAL SERVICE - INHIBITOR SWITCH CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| INHIBITOR SWITCH CONTINUITY CHECK
Item | Terminal No. | Resistance
--- | --- | ---
P | 3 - 8, 9 - 10 | Less than 2 Ω
R | 7 - 8
N | 4 - 8, 9 - 10
D | 1 - 8
NOTE: The inhibitor switch has 7 positions, but only four positions [P, R, N and D]are used.

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - ESSENTIAL SERVICE - INHIBITOR SWITCH CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation