[42] BODY - - WINDOW GLASS - ROOF WINDOW GLASS <Vehicles for Hong Kong spec> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ROOF WINDOW GLASS <Vehicles for Hong Kong spec>

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Frame assembly (Refer to GROUP 52A - Headlining ).
<<A>> | >>A<< | 1. | Roof window glass assembly
| REMOVAL SERVICE POINT
| <<A>> ROOF WINDOW GLASS ASSEMBLY REMOVAL Remove by the same procedure as for the quarter window glass (Refer to ).
| INSTALLATION SERVICE POINT
| >>A<< ROOF WINDOW GLASS ASSEMBLY INSTALLATION Install by the same procedure as for the windshield (Refer to ).

[42] BODY - - WINDOW GLASS - ROOF WINDOW GLASS <Vehicles for Hong Kong spec> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation