[42] BODY - - WINDOW GLASS - GENERAL | PRINT PAGE / INDEX / PRIOR / NEXT

| GENERAL
| The windshield, quarter window glass, tailgate window glass and roof window glass are attached by an urethane-base adhesive to the window frame. This adhesive provides improved glass holding and sealing, and also gives body openings a greater structural strength.
| ITEMS
Name | Remark
--- | ---
Adhesive | 3M ATD Part No. 8609 Super Fast Urethane Auto Glass Sealant or equivalent
Primer | 3M ATD Part No. 8608 Super Fast Urethane Primer or equivalent
Spacers | Available as service part
Dam | Available as service part
Anti-rust solvent (or Tectyl 506T...Valvoline Oil Company) | For rust prevention
Isopropyl alcohol | For grease removal from bonded surface
Steel piano wire | Dia. y length...0.6mm 1m For cutting adhesive
Glass adhesive knife | For cutting adhesive
Adhesive gun | For pressing-out adhesive
| HANDLING OF AUTO WINDOW SEALER Keep the sealant in a cool place, not exposed to the direct rays of the sun. Do not place any heavy article on the sealant nor press it, otherwise it will become deformed. Avoid storing the sealant for more than 6 months, because it will lose its sealing effect.
| BODY PINCH-WELD FLANGE SERVICING Before servicing the body pinch-weld flange, remove old adhesive completely. If the flange requires painting, bake it after painting is completed.
WINDOW GLASS INSTALLATION

[42] BODY - - WINDOW GLASS - GENERAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation