[54A] CHASSIS ELECTRICAL - - RHEOSTAT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| RHEOSTAT RESISTANCE CHECK
| Connect the battery and the test bulb (40 W) as shown in the illumination. Operate the rheostat, and if brightness changes smoothly without switching off, rheostat function is normal.

[54A] CHASSIS ELECTRICAL - - RHEOSTAT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation