[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR INSIDE HANDLE PLAY ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| DOOR INSIDE HANDLE PLAY ADJUSTMENT
| DOOR INSIDE HANDLE KNOB PLAY CHECK
| Check that the door inside handle knob play satisfies the standard value. Standard value (A): Driver’s side: 9.3 - 17.7 mm (target value: 13.9 mm) Except driver’s side: 3.8 - 12.2 mm (target value: 8.4 mm) Check the door inside handle and door latch assembly, and replace them if they are out of the standard value. Refer to .
| DOOR INSIDE HANDLE LOCK KNOB STROKE CHECK Removal the door trim assembly. Refer to GROUP 52A, Door Trim .
| Check that the stroke of the door inside handle lock knob satisfies the standard value. Standard value (A): Lock side: 3 - 5 mm Unlock side (Front door): 18 - 20 mm Unlock side (Rear door): 17 - 19 mm
| If it is outside the standard value, adjust the stroke of the inside handle lock knob by using the outer cable end, which connects the inside handle lock knob to the inside lock cable.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR INSIDE HANDLE PLAY ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation