[33] FRONT SUSPENSION - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
The front suspension is a McPherson strut with coil spring. The shock absorber is gas-filled hydraulic double-acting type.
CONSTRUCTION DIAGRAM
SPECIFICATIONS
COIL SPRING
Item | 2000 | 2400
--- | --- | ---
SOHC | DOHC | Vehicles for General Export (except for South Africa and Argentina), GCC, Australia (LS, XLS models) and New Zealand (LS, XLS models) | Vehicles for General Export (South Africa and Argentina) | Vehicles for Australia (LIMITED models) and New Zealand (LIMITED models)
Wire diameter mm | 14 | 14 | 14 | 14 | 14
Average diameter mm | 160 | 160 | 160 | 160 | 160
Free length mm | 328 | 325 | 347 | 305 | 353

[33] FRONT SUSPENSION - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation