[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - ON-VEHICLE SERVICE - SPARK PLUG CHECK AND CLEANING<4G69-MIVEC> | PRINT PAGE / INDEX / PRIOR / NEXT

| SPARK PLUG CHECK AND CLEANING<4G69-MIVEC> Remove the spark plugs. CAUTION Do not attempt to adjust the gap of the iridium plug. Always use a plug cleaner and finish cleaning within 20 seconds. Do not use wire brushes. Otherwise, the iridium tip may be damaged.
| Check the plug gap and replace if the limit is exceeded. Standard value: 0.7 - 0.8 mm Limit: 1.2 mm CAUTION Be careful not to allow foreign matter in cylinders. Clean the engine plug holes. Install the spark plugs.

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - ON-VEHICLE SERVICE - SPARK PLUG CHECK AND CLEANING<4G69-MIVEC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation