[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

HEATER CONTROL ASSEMBLY AND A/C SWITCH

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
| >>B<< | 1. | Air mix door cable connection
| >>A<< | 2. | Blower vent changeover damper cable connection
|  | 3. | Knob
|  | 4. | Centre panel
|  | 5. | Manual air conditioner control panel assembly
| INSTALLATION SERVICE POINT
| >>A<< BLOWER VENT CHANGEOVER DAMPER CABLE
| Set the heater control assembly’s blower vent changeover knob to the DEF position. Set the heater unit’s blower vent changeover damper relay to the DEF position (turn the damper relay to the left until it stops) and install the cable. Set the mode locator to the heater unit case and secure with a clip.
| >>B<< AIR MIX DOOR CABLE CONNECTION
| Turn the heater control assembly’s temperature adjustment knob all the way to the HOT side. Set the heater unit’s air mix door lever to the MAX HOT position (turn the damper lever as the left illustration) and attach the cable. Set the mode locator to the heater unit case and secure with a clip.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation