[37] POWER STEERING - - ON-VEHICLE SERVICE - STATIONARY STEERING EFFORT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| STATIONARY STEERING EFFORT CHECK With the vehicle stopped on a flat and paved surface, turn the steering wheel to the straight ahead position. Start the engine and set the engine idle speed. Standard value: 2000: 750 ± 100 r/min 2400: 700 ± 100 r/min
| Attach a spring balance to the outer circumference of the steering wheel and measure the steering force required to turn the steering wheel from the straight ahead position to the left and right (within a range of 1.5 turns). Also check to be sure that there is no significant change in the required steering effort. Standard value: Steering effort: 29 N or less Fluctuation allowance: 5.9 N or less If the measured value exceeds the standard value, check and adjust the related parts.

[37] POWER STEERING - - ON-VEHICLE SERVICE - STATIONARY STEERING EFFORT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation