[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - TRANSFER OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| TRANSFER OIL REPLACEMENT
| Remove the drain plug and discharge the oil. Tighten the drain plug to the specified torque. Tightening torque: 32 ± 2 N·m CAUTION Cover the heat protector of the front exhaust pipe with cardboard or something similar when refilling transfer oil so that transfer oil does not enter the area between the front exhaust pipe and heat protector. Remove the oil filer plug and pour in oil until it reaches the bottom the oil filer plug hole. Specified oil: Hypoid gear oil API classification GL-5 SAE 90 Quantity: 0.55 L Tighten the filler plug to the specified torque. Tightening torque: 32 ± 2 N·m

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - TRANSFER OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation