[3] WELDED PANEL REPLACEMENT - - QUARTER INNER | PRINT PAGE / INDEX / PRIOR / NEXT

QUARTER INNER
CAUTION When repairing the area using foam materials do not use firing tools since the foaming materials may burn. NOTE: Refer to the Quarter Outer section on for the welding points with the quarter outer.
| NOTE ON REPAIR WORK
| REMOVAL
| After assembling the quarter inner panel it is not possible to fill the inside of the rear pillar with foam materials. Thus, push in urethane foam (L45 mm x W60 mm x H60 mm) from the hole up to the dotted line to bury the inside of the rear pillar, as shown in the figure of the instructions.

[3] WELDED PANEL REPLACEMENT - - QUARTER INNER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation