[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ENGINE-A/T-ECU - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ENGINE-A/T-ECU

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Cowl Side Trim (RH) Removal and Installation <LH Drive vehicles> (Refer to GROUP 52A, Instrument Panel Assembly ). Instrument Panel Console Side Cover (LH) Removal and Installation <RH Drive vehicles> (Refer to GROUP 52A, Instrument Panel Assembly ).
|  |  | REMOVAL STEPS
--- | --- | --- | ---
|  | 1. | Floor console front bracket <RH Drive vehicles>
|  | 2. | Engine-A/T-ECU connector
|  | 3. | Engine-A/T-ECU
|  | 4. | Engine-A/T-ECU bracket

[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ENGINE-A/T-ECU - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation