[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A3. CHECK IGNITION CABLES FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

| A3. CHECK IGNITION CABLES FOR DAMAGE
| Check the ignition cable and rubber cap for damage or weakness, and check the installation condition. Check the ignition cable and spark plug, distributor, and ignition coil connections for contamination, dirt, etc. If dirty, clean it; if damaged, replace it.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A3. CHECK IGNITION CABLES FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation