[23] AUTOMATIC TRANSMISSION - - ELECTRONIC CONTROL SYSTEM - DIAGNOSIS CLASSIFICATION TABLE <4G63, 4G64> | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSIS CLASSIFICATION TABLE <4G63, 4G64>
Item | Diagnosis code No. | Data list | Actuator test
--- | --- | --- | ---
Item No. | Display
Throttle position sensor (TPS) | Short circuit | 11 | 11 | mV | -
Open circuit | 12 | -
Sensor maladjustment | 14 | -
A/T fluid temperature sensor | Open circuit | 15 | 15 | °C | -
Crank angle sensor | Open circuit | 21 | 21 <4G64> 00 <4G63> | r/min | -
Input shaft speed sensor | Short circuit/open circuit | 22 | 22 <4G64> 01 <4G63> | r/min | -
Output shaft speed sensor | Short circuit/open circuit | 23 | 23 <4G64> 02 <4G63> | r/min | -
Stop lamp switch | Short circuit | 26 | 26 | ON/OFF | -
Vehicle speed signal | - | 29 | km/h | -
LR solenoid valve | Short circuit/open circuit | 31 | 31 | % | 01
UD solenoid valve | Short circuit/open circuit | 32 | 32 | % | 02
2ND solenoid valve | Short circuit/open circuit | 33 | 33 | % | 03
OD solenoid valve | Short circuit/open circuit | 34 | 34 | % | 04
RED solenoid valve <5A/T> | Short circuit/open circuit | 35 | 35 | % | 05
DCC solenoid valve | Short circuit/open circuit | 36 | 36 | % | 06
Gear shift incomplete | 1st | 41 | - | - | -
2nd | 42 | - | - | -
3rd | 43 | - | - | -
4th | 44 | - | - | -
5th <5A/T> | 45 | - | - | -
Reverse | 46 | - | - | -
Damper clutch system | System defect | 52 | 52 | r/min | -
A/T control relay | Earth short circuit/open circuit | 54 | 54 | V | 12
"N" range lamp | Open circuit | 56 | - | - | -
Engine volumetric efficiency | - | 57 | % | -
Inhibitor switch | - | 61 | P, R, N, D | -
Shift position | - | 63 | 5th <5A/T>, 4th, 3rd, 2nd, 1st, REV, NP | -
A/C-ECU | - | 65 | ON/OFF | -
Auto-cruise engaged signal | - | 66 | ON/OFF | -
Select switch | - | 67 | ON/OFF | -
Shift switch (Up) | - | 68 | ON/OFF | -
Shift switch (Down) | - | 69 | ON/OFF | -
Steering shift switch <5A/T> | - | 70 | mV | -
Shift indicator | 1st | - | - | - | 07
2nd | - | - | - | 08
3rd | - | - | - | 09
4th | - | - | - | 10
5th <5A/T> | - | - | - | 11
INVECS-II cancel command | - | - | - | 14
Downshift forbidden buzzer <5A/T> | - | - | - | 15

[23] AUTOMATIC TRANSMISSION - - ELECTRONIC CONTROL SYSTEM - DIAGNOSIS CLASSIFICATION TABLE <4G63, 4G64> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation