[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND ASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Switch panel
|  | 2. | Rear window defogger switch
|  | 3. | Air conditioner switch
|  | 4. | Inside/outside air selection switch
| <<A>> | 5. | Blower vent changeover damper cable
| <<A>> | 6. | Air mix damper cable
|  | 7. | Blower switch assembly
|  | 8. | Manual air conditioner control panel (A/C-ECU)
| DISASSEMBLY SERVICE POINT
| <<A>> BLOW VENT CHANGEOVER DAMPER CABLE AND AIR MIX DAMPER CABLE REMOVAL
| Insert a flat-tipped screwdriver into the clip through the inside of the control base and prize out the clip claw to disconnect the cables.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation